

CPVC 90 Degree Elbow

F

Submittal Information

* Standard Size Elbows Fabricated From Seamless
* Extruded CPVC Duct
* All Fitting Dimensions Based on 1:1 Fitting Ratio
* Fitting Segments Triple-Pass Welded Using 5/32” CPVC Welding Rod
* All Dimensions In Inches
* All Dimensions are to CSSI Standards and are Subject to Change

 90 Degree Elbow-5 pieces

PRODUCT DIMENSIONS

|  |
| --- |
|  |

CPVC 90 DEGREE ELBOW SUBMITTAL INFORMATION

90

A

Model Number Nominal Duct Size Average Duct O.D. A B Average Wall End Type

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  Thickness  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 90-CPVC-6-1 | 6 | 6.625 | 6.625 | A+2" | 0.187 |
| 90-CPVC-7-1 | 7 | 7.375 | 7.375 | A+2" | 0.187 |
| 90-CPVC-8-1 | 8 | 8.625 | 8.625 | A+2" | 0.187 |
| 90-CPVC-9-1 | 9 | 9.375 | 9.375 | A+2" | 0.187 |
| 90-CPVC-10-1 | 10 | 10.75 | 10.75 | A+2" | 0.187 |
| 90-CPVC-12-1 | 12 | 12.75 | 12.75 | A+2" | 0.187 |
| 90-CPVC-14-1 | 14 | 14 | 14 | A+2" | 0.187 |
| 90-CPVC-16-1 | 16 | 16 | 16 | A+2" | 0.187 |
| 90-CPVC-18-1 | 18 | 18 | 18 | A+2" | 0.187 |
| 90-CPVC-20-1 | 20 | 20 | 20 | A+3" | 0.219 |
| 90-CPVC-24-1 | 24 | 24 | 24 | A+3" | 0.25 |

SOCKET

“B” END TYPE